**Truma Combi 6 and 6E Technical Data**

|  |  |  |  |
| --- | --- | --- | --- |
| **Technical Data** |  | **Combi 6** | **Combi 6E** |
| Water capacity | (litres) | 10 | 10 |
| Time to heat water from about 15⁰C to 60⁰C | | | |
| Water heating only, Gas, Boost | minutes | 20 | 20 |
| Water heating only, EL 2 | minutes | N/A | 45 |
| Water and room heating, Gas | minutes | 80 | 80 |
| Water and room heating, Mix 2 |  | N/A | 60 |
| Gas consumption | gm/hr | 160 – 480 | 160 – 480 |
| Max air delivery volume | mᶟ/hr | 287 | 287 |
| Current consumption during operation 12V | A | Approx 1.3 | Approx 1.3 |
| Stand-by current consumption | A | <0.001 | <0.001 |